Cold moulding is similar to FRP in as much as it involves the use of epoxy or polyester resins, but the structural component is wood instead of fibreglass. In cold moulding very thin strips of wood are
